MIKROTIK-MIB DEFINITIONS ::= BEGIN

IMPORTS
InetAddressType, InetAddress, InetPortNumber FROM INET-ADDRESS-MIB
MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Gauge32, IpAddress,
Counter64, enterprises, NOTIFICATION-TYPE, TimeTicks FROM SNMPv2-SMI
TEXTUAL-CONVENTION, DisplayString, MacAddress, TruthValue, DateAndTime FROM SNMPv2-TC
OBJECT-GROUP, NOTIFICATION-GROUP FROM SNMPv2-CONF;

mikrotikExperimentalModule MODULE-IDENTITY
  LAST-UPDATED "202505190000Z"
  ORGANIZATION "MikroTik"
  CONTACT-INFO "support@mikrotik.com"
  DESCRIPTION ""
  REVISION "202505190000Z"
  DESCRIPTION ""
  ::= { mikrotik 1 }

mikrotik OBJECT IDENTIFIER ::= { enterprises 14988 }
mtXMetaInfo OBJECT IDENTIFIER ::= { mikrotikExperimentalModule 2 }
mtXRouterOsGroups OBJECT IDENTIFIER ::= { mtXMetaInfo 1 }

mtXRouterOs OBJECT IDENTIFIER ::= { mikrotikExperimentalModule 1 }
mtxrWireless OBJECT IDENTIFIER ::= { mtXRouterOs 1 }
mtxrQueues OBJECT IDENTIFIER ::= { mtXRouterOs 2 }
mtxrHealth OBJECT IDENTIFIER ::= { mtXRouterOs 3 }
mtxrLicense OBJECT IDENTIFIER ::= { mtXRouterOs 4 }
mtxrHotspot OBJECT IDENTIFIER ::= { mtXRouterOs 5 }
mtxrDHCP OBJECT IDENTIFIER ::= { mtXRouterOs 6 }
mtxrSystem OBJECT IDENTIFIER ::= { mtXRouterOs 7 }
mtxrScripts OBJECT IDENTIFIER ::= { mtXRouterOs 8 }
mtxrTraps OBJECT IDENTIFIER ::= { mtXRouterOs 9 }
mtxrNstremeDual OBJECT IDENTIFIER ::= { mtXRouterOs 10 }
mtxrNeighbor OBJECT IDENTIFIER ::= { mtXRouterOs 11 }
mtxrGps OBJECT IDENTIFIER ::= { mtXRouterOs 12 }
mtxrWirelessModem OBJECT IDENTIFIER ::= { mtXRouterOs 13 }
mtxrInterfaceStats OBJECT IDENTIFIER ::= { mtXRouterOs 14 }
mtxrPOE OBJECT IDENTIFIER ::= { mtXRouterOs 15 }
mtxrLTEModem OBJECT IDENTIFIER ::= { mtXRouterOs 16 }
mtxrPartition OBJECT IDENTIFIER ::= { mtXRouterOs 17 }
mtxrScriptRun OBJECT IDENTIFIER ::= { mtXRouterOs 18 }
mtxrOptical OBJECT IDENTIFIER ::= { mtXRouterOs 19 }
mtxrIPSec OBJECT IDENTIFIER ::= { mtXRouterOs 20 }
mtxrWifi OBJECT IDENTIFIER ::= { mtXRouterOs 21 }
mtxrCT OBJECT IDENTIFIER ::= { mtXRouterOs 22 }

ObjectIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS current
    DESCRIPTION "Internal "
    SYNTAX Integer32 (0..2147483647)
-- Note that actually in RouterOs index values can be in range 0..4294967294,
-- this can sometimes make them negative. Any of the following syntaxes would
-- be more appropriate, but since Integer32 is used for InterfaceIndex in
-- IF-MIB, where it can also take negative values in RouterOs, it is used
-- here for consistency.
-- Also note that ObjectIndex value is not related to item numbers that are
-- used by console and shown by console print command.
--
-- SYNTAX Integer32 (-2147483648..2147483647)
-- SYNTAX Unsigned32 (0..4294967295)

HexInt ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS current
    DESCRIPTION "Hex"
    SYNTAX Integer32 (-2147483648..2147483647)

Voltage ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS current
    DESCRIPTION ""
    SYNTAX Integer32 (-2147483648..2147483647)

Temperature ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS current
    DESCRIPTION ""
    SYNTAX Integer32 (-2147483648..2147483647)

Power ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS current
    DESCRIPTION ""
    SYNTAX Integer32 (-2147483648..2147483647)

GDiv100 ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-2"
    STATUS current
    DESCRIPTION "/100"
    SYNTAX Gauge32

GDiv1000 ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-3"
    STATUS current
    DESCRIPTION "/1000"
    SYNTAX Gauge32

IDiv1000 ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-3"
    STATUS current
    DESCRIPTION "/1000"
    SYNTAX Integer32 (-2147483648..2147483647)

BoolValue ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
    "Boolean value."
    SYNTAX       INTEGER { false(0), true(1) }

IsakmpCookie ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "16a"
    STATUS          current
    DESCRIPTION "ISAKMP cookie string"
    SYNTAX  OCTET STRING (SIZE (16))

-- WIRELESS ********************************************************************

mtxrWlStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 1 }

mtxrWlStatEntry OBJECT-TYPE
    SYNTAX MtxrWlStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless station mode interface"
    INDEX { mtxrWlStatIndex }
    ::= { mtxrWlStatTable 1 }

MtxrWlStatEntry ::= SEQUENCE {
    mtxrWlStatIndex ObjectIndex,
    mtxrWlStatTxRate Gauge32,
    mtxrWlStatRxRate Gauge32,
    mtxrWlStatStrength Integer32,
    mtxrWlStatSsid DisplayString,
    mtxrWlStatBssid MacAddress,
    mtxrWlStatFreq Integer32,
    mtxrWlStatBand DisplayString,
    mtxrWlStatTxCCQ Counter32,
    mtxrWlStatRxCCQ Counter32
}

mtxrWlStatIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 1 }

mtxrWlStatTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlStatEntry 2 }

mtxrWlStatRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlStatEntry 3 }

mtxrWlStatStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrWlStatEntry 4 }

mtxrWlStatSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 5 }

mtxrWlStatBssid OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 6 }

mtxrWlStatFreq OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "megahertz"
    ::= { mtxrWlStatEntry 7 }

mtxrWlStatBand OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 8 }

mtxrWlStatTxCCQ OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 9 }

mtxrWlStatRxCCQ OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 10 }

-- WlRtabTable
mtxrWlRtabTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlRtabEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 2 }

mtxrWlRtabEntry OBJECT-TYPE
    SYNTAX MtxrWlRtabEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless registration table. It is indexed by remote
        mac-address and local interface index"
    INDEX { mtxrWlRtabAddr, mtxrWlRtabIface }
    ::= { mtxrWlRtabTable 1 }

MtxrWlRtabEntry ::= SEQUENCE {
    mtxrWlRtabAddr MacAddress,
    mtxrWlRtabIface ObjectIndex,
    mtxrWlRtabStrength Integer32,
    mtxrWlRtabTxBytes Counter32,
    mtxrWlRtabRxBytes Counter32,
    mtxrWlRtabTxPackets Counter32,
    mtxrWlRtabRxPackets Counter32,
    mtxrWlRtabTxRate Gauge32,
    mtxrWlRtabRxRate Gauge32,
    mtxrWlRtabRouterOSVersion DisplayString,
    mtxrWlRtabUptime TimeTicks,
    mtxrWlRtabSignalToNoise Integer32,
    mtxrWlRtabTxStrengthCh0 Integer32,
    mtxrWlRtabRxStrengthCh0 Integer32,
    mtxrWlRtabTxStrengthCh1 Integer32,
    mtxrWlRtabRxStrengthCh1 Integer32,
    mtxrWlRtabTxStrengthCh2 Integer32,
    mtxrWlRtabRxStrengthCh2 Integer32,
    mtxrWlRtabTxStrength Integer32,
    mtxrWlRtabRadioName DisplayString
}

mtxrWlRtabAddr OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 1 }

mtxrWlRtabIface OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 2 }

mtxrWlRtabStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrWlRtabEntry 3 }

mtxrWlRtabTxBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 4 }

mtxrWlRtabRxBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 5 }

mtxrWlRtabTxPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 6 }

mtxrWlRtabRxPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 7 }

mtxrWlRtabTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlRtabEntry 8 }

mtxrWlRtabRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlRtabEntry 9 }

mtxrWlRtabRouterOSVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "RouterOS version"
    ::= { mtxrWlRtabEntry 10 }

mtxrWlRtabUptime OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "uptime"
    ::= { mtxrWlRtabEntry 11 }

mtxrWlRtabSignalToNoise OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Measured in dB, if value does not exist it is indicated with 0"
    ::= { mtxrWlRtabEntry 12 }

mtxrWlRtabTxStrengthCh0 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 13 }

mtxrWlRtabRxStrengthCh0 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 14 }

mtxrWlRtabTxStrengthCh1 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 15 }

mtxrWlRtabRxStrengthCh1 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 16 }

mtxrWlRtabTxStrengthCh2 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 17 }

mtxrWlRtabRxStrengthCh2 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 18 }

mtxrWlRtabTxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 19 }

mtxrWlRtabRadioName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 20 }

mtxrWlRtabEntryCount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Wireless registration table entry count"
    ::= { mtxrWireless 4 }

mtxrWlApTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlApEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 3 }

mtxrWlApEntry OBJECT-TYPE
    SYNTAX MtxrWlApEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless access point mode interface"
    INDEX { mtxrWlApIndex }
    ::= { mtxrWlApTable 1 }

MtxrWlApEntry ::= SEQUENCE {
    mtxrWlApIndex ObjectIndex,
    mtxrWlApTxRate Gauge32,
    mtxrWlApRxRate Gauge32,
    mtxrWlApSsid DisplayString,
    mtxrWlApBssid MacAddress,
    mtxrWlApClientCount Counter32,
    mtxrWlApFreq Integer32,
    mtxrWlApBand DisplayString,
    mtxrWlApNoiseFloor Integer32,
    mtxrWlApOverallTxCCQ Counter32,
    mtxrWlApAuthClientCount Counter32
}

mtxrWlApIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 1 }

mtxrWlApTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlApEntry 2 }

mtxrWlApRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlApEntry 3 }

mtxrWlApSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 4 }

mtxrWlApBssid OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 5 }

mtxrWlApClientCount OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 6 }

mtxrWlApFreq OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "megahertz"
    ::= { mtxrWlApEntry 7 }

mtxrWlApBand OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 8 }

mtxrWlApNoiseFloor OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 9 }

mtxrWlApOverallTxCCQ OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 10 }

mtxrWlApAuthClientCount OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 11 }

mtxrWlCMRtabTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlCMRtabEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 5 }

mtxrWlCMRtabEntry OBJECT-TYPE
    SYNTAX MtxrWlCMRtabEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless CAPSMAN registration table. It is indexed by remote
        mac-address and local interface index"
    INDEX { mtxrWlCMRtabAddr, mtxrWlCMRtabIface }
    ::= { mtxrWlCMRtabTable 1 }

MtxrWlCMRtabEntry ::= SEQUENCE {
    mtxrWlCMRtabAddr MacAddress,
    mtxrWlCMRtabIface ObjectIndex,
    mtxrWlCMRtabUptime TimeTicks,
    mtxrWlCMRtabTxBytes Counter32,
    mtxrWlCMRtabRxBytes Counter32,
    mtxrWlCMRtabTxPackets Counter32,
    mtxrWlCMRtabRxPackets Counter32,
    mtxrWlCMRtabTxRate Gauge32,
    mtxrWlCMRtabRxRate Gauge32,
    mtxrWlCMRtabTxStrength Integer32,
    mtxrWlCMRtabRxStrength Integer32,
    mtxrWlCMRtabSsid DisplayString,
    mtxrWlCMRtabEapIdent DisplayString
}

mtxrWlCMRtabAddr OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 1 }
    -- should not be accessible in SMIv2

mtxrWlCMRtabIface OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 2 }

mtxrWlCMRtabUptime OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "uptime"
    ::= { mtxrWlCMRtabEntry 3 }

mtxrWlCMRtabTxBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 4 }

mtxrWlCMRtabRxBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 5 }

mtxrWlCMRtabTxPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 6 }

mtxrWlCMRtabRxPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 7 }

mtxrWlCMRtabTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlCMRtabEntry 8 }

mtxrWlCMRtabRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlCMRtabEntry 9 }

mtxrWlCMRtabTxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 10 }

mtxrWlCMRtabRxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 11 }

mtxrWlCMRtabSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 12 }

mtxrWlCMRtabEapIdent OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRtabEntry 13 }

mtxrWlCMRtabEntryCount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Wireless CAPSMAN registration table entry count"
    ::= { mtxrWireless 6 }

mtxrWlCMREntryCount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Wireless CAPSMAN remote-cap entry count"
    ::= { mtxrWireless 10 }

mtxrWlCMTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlCMEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 7 }

mtxrWlCMEntry OBJECT-TYPE
    SYNTAX MtxrWlCMEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "CAPS-MAN mode interface"
    INDEX { mtxrWlCMIndex }
    ::= { mtxrWlCMTable 1 }

MtxrWlCMEntry ::= SEQUENCE {
    mtxrWlCMIndex ObjectIndex,
    mtxrWlCMRegClientCount Counter32,
    mtxrWlCMAuthClientCount Counter32,
    mtxrWlCMState DisplayString,
    mtxrWlCMChannel DisplayString
}

mtxrWlCMIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMEntry 1 }

mtxrWlCMRegClientCount OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMEntry 2 }

mtxrWlCMAuthClientCount OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMEntry 3 }

mtxrWlCMState OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMEntry 4 }

mtxrWlCMChannel OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "for master only"
    ::= { mtxrWlCMEntry 5 }

--
mtxrWlCMRemoteTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlCMRemoteEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 11 }

mtxrWlCMRemoteEntry OBJECT-TYPE
    SYNTAX MtxrWlCMRemoteEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "CAPSMAN remote-cap list"
    INDEX { mtxrWlCMRemoteIndex }
    ::= { mtxrWlCMRemoteTable 1 }

MtxrWlCMRemoteEntry ::= SEQUENCE {
    mtxrWlCMRemoteIndex ObjectIndex,
    mtxrWlCMRemoteName DisplayString,
    mtxrWlCMRemoteState DisplayString,
    mtxrWlCMRemoteAddress DisplayString,
    mtxrWlCMRemoteRadios Counter32
}

mtxrWlCMRemoteIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRemoteEntry 1 }

mtxrWlCMRemoteName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRemoteEntry 2 }

mtxrWlCMRemoteState OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRemoteEntry 3 }

mtxrWlCMRemoteAddress OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRemoteEntry 4 }

mtxrWlCMRemoteRadios OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlCMRemoteEntry 5 }

-- W60G
mtxrWl60GTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWl60GEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 8 }

mtxrWl60GEntry OBJECT-TYPE
    SYNTAX MtxrWl60GEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "W60G interface"
    INDEX { mtxrWl60GIndex }
    ::= { mtxrWl60GTable 1 }

MtxrWl60GEntry ::= SEQUENCE {
    mtxrWl60GIndex ObjectIndex,
    mtxrWl60GMode INTEGER,
    mtxrWl60GSsid DisplayString,
    mtxrWl60GConnected BoolValue,
    mtxrWl60GRemote MacAddress,
    mtxrWl60GFreq Integer32,
    mtxrWl60GMcs Integer32,
    mtxrWl60GSignal Integer32,
    mtxrWl60GTxSector Integer32,
    mtxrWl60GTxSectorInfo DisplayString,
    mtxrWl60GRssi Integer32,
    mtxrWl60GPhyRate Gauge32
}

mtxrWl60GIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 1 }

mtxrWl60GMode OBJECT-TYPE
    SYNTAX INTEGER {
        apBridge(0),
        stationBridge(1),
        sniff(2),
        bridge(3)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 2 }

mtxrWl60GSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 3 }

mtxrWl60GConnected OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 4 }

mtxrWl60GRemote OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 5 }

mtxrWl60GFreq OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Mhz"
    ::= { mtxrWl60GEntry 6 }

mtxrWl60GMcs OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 7 }

mtxrWl60GSignal OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 8 }

mtxrWl60GTxSector OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 9 }

mtxrWl60GTxSectorInfo OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 11 }

mtxrWl60GRssi OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 12 }

mtxrWl60GPhyRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GEntry 13 }

-- W60GSta
mtxrWl60GStaTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWl60GStaEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 9 }

mtxrWl60GStaEntry OBJECT-TYPE
    SYNTAX MtxrWl60GStaEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "W60G stations"
    INDEX { mtxrWl60GStaIndex }
    ::= { mtxrWl60GStaTable 1 }

MtxrWl60GStaEntry ::= SEQUENCE {
    mtxrWl60GStaIndex ObjectIndex,
    mtxrWl60GStaConnected BoolValue,
    mtxrWl60GStaRemote MacAddress,
    mtxrWl60GStaMcs Integer32,
    mtxrWl60GStaSignal Integer32,
    mtxrWl60GStaTxSector Integer32,
    mtxrWl60GStaPhyRate Gauge32,
    mtxrWl60GStaRssi Integer32,
    mtxrWl60GStaDistance Integer32
}

mtxrWl60GStaIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 1 }

mtxrWl60GStaConnected OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 2 }

mtxrWl60GStaRemote OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 3 }

mtxrWl60GStaMcs OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 4 }

mtxrWl60GStaSignal OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 5 }

mtxrWl60GStaTxSector OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 6 }

mtxrWl60GStaPhyRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Mbits per second"
    ::= { mtxrWl60GStaEntry 8 }

mtxrWl60GStaRssi OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWl60GStaEntry 9 }

mtxrWl60GStaDistance OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "meters"
    ::= { mtxrWl60GStaEntry 10 }


mtxrWirelessGroup OBJECT-GROUP OBJECTS {
        mtxrWlStatTxRate,
	mtxrWlStatRxRate,
	mtxrWlStatStrength,
	mtxrWlStatSsid,
        mtxrWlStatBssid,
	mtxrWlStatFreq,
	mtxrWlStatBand,
        mtxrWlStatTxCCQ,
        mtxrWlStatRxCCQ,
	mtxrWlRtabStrength,
	mtxrWlRtabTxBytes,
        mtxrWlRtabRxBytes,
	mtxrWlRtabTxPackets,
	mtxrWlRtabRxPackets,
        mtxrWlRtabTxRate,
	mtxrWlRtabRxRate,
	mtxrWlRtabEntryCount,
        mtxrWlRtabRouterOSVersion,
        mtxrWlRtabUptime,
        mtxrWlRtabSignalToNoise,
        mtxrWlRtabTxStrengthCh0,
        mtxrWlRtabRxStrengthCh0,
        mtxrWlRtabTxStrengthCh1,
        mtxrWlRtabRxStrengthCh1,
        mtxrWlRtabTxStrengthCh2,
        mtxrWlRtabRxStrengthCh2,
        mtxrWlRtabTxStrength,
        mtxrWlRtabRadioName,
        mtxrWlApTxRate,
	mtxrWlApRxRate,
	mtxrWlApSsid,
        mtxrWlApBssid,
        mtxrWlApClientCount,
        mtxrWlApBand,
        mtxrWlApFreq,
        mtxrWlApNoiseFloor,
        mtxrWlApOverallTxCCQ,
        mtxrWlApAuthClientCount,
        mtxrWlCMRtabAddr,
        mtxrWlCMRtabTxBytes,
        mtxrWlCMRtabRxBytes,
        mtxrWlCMRtabTxPackets,
        mtxrWlCMRtabRxPackets,
        mtxrWlCMRtabTxRate,
        mtxrWlCMRtabRxRate,
        mtxrWlCMRtabUptime,
        mtxrWlCMRtabTxStrength,
        mtxrWlCMRtabRxStrength,
        mtxrWlCMRtabSsid,
        mtxrWlCMRtabEntryCount,
        mtxrWlCMREntryCount,
        mtxrWlCMRegClientCount,
        mtxrWlCMAuthClientCount,
        mtxrWl60GMode,
        mtxrWl60GSsid,
        mtxrWl60GConnected,
        mtxrWl60GRemote,
        mtxrWl60GFreq,
        mtxrWl60GMcs,
        mtxrWl60GSignal,
        mtxrWl60GTxSector,
        mtxrWl60GTxSectorInfo,
        mtxrWl60GRssi,
        mtxrWl60GPhyRate,
        mtxrWl60GStaConnected,
        mtxrWl60GStaRemote,
        mtxrWl60GStaMcs,
        mtxrWl60GStaSignal,
        mtxrWl60GStaTxSector
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 1 }

-- QUEUES ********************************************************************

mtxrQueueSimpleTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrQueueSimpleEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueues 1 }

mtxrQueueSimpleEntry OBJECT-TYPE
    SYNTAX MtxrQueueSimpleEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Simple queue"
    INDEX { mtxrQueueSimpleIndex }
    ::= { mtxrQueueSimpleTable 1 }

MtxrQueueSimpleEntry ::= SEQUENCE {
    mtxrQueueSimpleIndex ObjectIndex,
    mtxrQueueSimpleName DisplayString,
    mtxrQueueSimpleSrcAddr IpAddress,
    mtxrQueueSimpleSrcMask IpAddress,
    mtxrQueueSimpleDstAddr IpAddress,
    mtxrQueueSimpleDstMask IpAddress,
    mtxrQueueSimpleIface ObjectIndex,
    mtxrQueueSimpleBytesIn Counter64,
    mtxrQueueSimpleBytesOut Counter64,
    mtxrQueueSimplePacketsIn Counter32,
    mtxrQueueSimplePacketsOut Counter32,
    mtxrQueueSimplePCQQueuesIn Counter32,
    mtxrQueueSimplePCQQueuesOut Counter32,
    mtxrQueueSimpleDroppedIn Counter32,
    mtxrQueueSimpleDroppedOut Counter32
}

mtxrQueueSimpleIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 1 }

mtxrQueueSimpleName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 2 }

mtxrQueueSimpleSrcAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 3 }

mtxrQueueSimpleSrcMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 4 }

mtxrQueueSimpleDstAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 5 }

mtxrQueueSimpleDstMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 6 }

mtxrQueueSimpleIface OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "interface index"
    ::= { mtxrQueueSimpleEntry 7 }

mtxrQueueSimpleBytesIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 8 }

mtxrQueueSimpleBytesOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 9 }

mtxrQueueSimplePacketsIn OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 10 }

mtxrQueueSimplePacketsOut OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 11 }

mtxrQueueSimplePCQQueuesIn OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 12 }

mtxrQueueSimplePCQQueuesOut OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 13 }

mtxrQueueSimpleDroppedIn OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 14 }

mtxrQueueSimpleDroppedOut OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 15 }

mtxrQueueTreeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrQueueTreeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueues 2 }

mtxrQueueTreeEntry OBJECT-TYPE
    SYNTAX MtxrQueueTreeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Tree queue"
    INDEX { mtxrQueueTreeIndex }
    ::= { mtxrQueueTreeTable 1 }

MtxrQueueTreeEntry ::= SEQUENCE {
    mtxrQueueTreeIndex ObjectIndex,
    mtxrQueueTreeName DisplayString,
    mtxrQueueTreeFlow DisplayString,
    mtxrQueueTreeParentIndex ObjectIndex,
    mtxrQueueTreeBytes Counter32,
    mtxrQueueTreePackets Counter32,
    mtxrQueueTreeHCBytes Counter64,
    mtxrQueueTreePCQQueues Counter32,
    mtxrQueueTreeDropped Counter32
}

mtxrQueueTreeIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 1 }

mtxrQueueTreeName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 2 }

mtxrQueueTreeFlow OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "flowmark"
    ::= { mtxrQueueTreeEntry 3 }

mtxrQueueTreeParentIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "index of parent tree queue or parent interface"
    ::= { mtxrQueueTreeEntry 4 }

mtxrQueueTreeBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 5 }

mtxrQueueTreePackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 6 }

mtxrQueueTreeHCBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 7 }

mtxrQueueTreePCQQueues OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 8 }

mtxrQueueTreeDropped OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 9 }

mtxrQueueGroup OBJECT-GROUP OBJECTS {
        mtxrQueueSimpleName, mtxrQueueSimpleSrcAddr, mtxrQueueSimpleSrcMask,
        mtxrQueueSimpleDstAddr, mtxrQueueSimpleDstMask, mtxrQueueSimpleIface,
        mtxrQueueSimpleBytesIn, mtxrQueueSimpleBytesOut,
        mtxrQueueSimplePacketsIn, mtxrQueueSimplePacketsOut, mtxrQueueTreeName,
        mtxrQueueSimplePCQQueuesIn,
        mtxrQueueSimplePCQQueuesOut,
        mtxrQueueSimpleDroppedIn,
        mtxrQueueSimpleDroppedOut,
        mtxrQueueTreeFlow, mtxrQueueTreeParentIndex, mtxrQueueTreeBytes,
        mtxrQueueTreePackets,
        mtxrQueueTreeHCBytes,
        mtxrQueueTreePCQQueues,
        mtxrQueueTreeDropped
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 2 }

-- HEALTH ********************************************************************

mtxrHlCoreVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "core voltage"
    ::= { mtxrHealth 1 }

mtxrHlThreeDotThreeVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "3.3V voltage"
    ::= { mtxrHealth 2 }

mtxrHlFiveVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "5V voltage"
    ::= { mtxrHealth 3 }

mtxrHlTwelveVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "12V voltage"
    ::= { mtxrHealth 4 }

mtxrHlSensorTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "temperature at sensor chip"
    ::= { mtxrHealth 5 }

mtxrHlCpuTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "temperature near cpu"
    ::= { mtxrHealth 6 }

mtxrHlBoardTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 7 }

mtxrHlVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 8 }

mtxrHlActiveFan OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 9 }

mtxrHlTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 10 }

mtxrHlProcessorTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 11 }

mtxrHlPower OBJECT-TYPE
    SYNTAX Power
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Watts"
    ::= { mtxrHealth 12 }

mtxrHlCurrent OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "mA"
    ::= { mtxrHealth 13 }

mtxrHlProcessorFrequency OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Mhz"
    ::= { mtxrHealth 14 }

mtxrHlPowerSupplyState OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "PSU state ok"
    ::= { mtxrHealth 15 }

mtxrHlBackupPowerSupplyState OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "backup PSU state ok"
    ::= { mtxrHealth 16 }

mtxrHlFanSpeed1 OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "rpm"
    ::= { mtxrHealth 17 }

mtxrHlFanSpeed2 OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "rpm"
    ::= { mtxrHealth 18 }

mtxrAlarmSocketStatus OBJECT-TYPE
    SYNTAX INTEGER {
        inactive(0),
        active(1)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Alarm socket status"
    ::= { mtxrHealth 19 }

mtxrGaugeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrGaugeTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 100 }

mtxrGaugeTableEntry OBJECT-TYPE
    SYNTAX MtxrGaugeTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrGaugeIndex }
    ::= { mtxrGaugeTable 1 }

MtxrGaugeTableEntry ::= SEQUENCE {
    mtxrGaugeIndex ObjectIndex,
    mtxrGaugeName DisplayString,
    mtxrGaugeValue Integer32,
    mtxrGaugeUnit INTEGER
}

mtxrGaugeIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrGaugeTableEntry 1 }

mtxrGaugeName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrGaugeTableEntry 2 }

mtxrGaugeValue OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrGaugeTableEntry 3 }

mtxrGaugeUnit OBJECT-TYPE
    SYNTAX INTEGER {
        celsius(1),
        rpm(2),
        dV(3),
        dA(4),
        dW(5),
        status(6)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "units"
    ::= { mtxrGaugeTableEntry 4 }

mtxrHealthGroup OBJECT-GROUP OBJECTS {
        mtxrHlCoreVoltage, mtxrHlThreeDotThreeVoltage, mtxrHlFiveVoltage,
        mtxrHlTwelveVoltage, mtxrHlSensorTemperature, mtxrHlCpuTemperature,
        mtxrHlBoardTemperature, mtxrHlVoltage, mtxrHlActiveFan, 
	mtxrHlTemperature, mtxrHlProcessorTemperature,
        mtxrHlCurrent, mtxrHlPower,
        mtxrHlProcessorFrequency,
        mtxrHlPowerSupplyState, mtxrHlBackupPowerSupplyState,
        mtxrHlFanSpeed1, mtxrHlFanSpeed2, mtxrAlarmSocketStatus,
        mtxrGaugeName, mtxrGaugeValue, mtxrGaugeUnit
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 3 }

-- LICENSE ********************************************************************

mtxrLicSoftwareId OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "software id"
    ::= { mtxrLicense 1 }

mtxrLicUpgrUntil OBJECT-TYPE
    SYNTAX DateAndTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "current key allows upgrading until this date"
    ::= { mtxrLicense 2 }

mtxrLicLevel OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "current key level"
    ::= { mtxrLicense 3 }

mtxrLicVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "software version"
    ::= { mtxrLicense 4 }

mtxrLicUpgradableTo OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "upgradable to"
    ::= { mtxrLicense 5 }

mtxrLincenseGroup OBJECT-GROUP OBJECTS {
        mtxrLicSoftwareId, mtxrLicUpgrUntil, mtxrLicLevel, mtxrLicVersion, mtxrLicUpgradableTo
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 4 }

-- HOTSPOT ***************************************************************

mtxrHotspotActiveUsersTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrHotspotActiveUsersTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspot 1 }

mtxrHotspotActiveUsersTableEntry OBJECT-TYPE
    SYNTAX MtxrHotspotActiveUsersTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrHotspotActiveUserIndex }
    ::= { mtxrHotspotActiveUsersTable 1 }

MtxrHotspotActiveUsersTableEntry ::= SEQUENCE {
	mtxrHotspotActiveUserIndex ObjectIndex,
	mtxrHotspotActiveUserServerID Integer32,
	mtxrHotspotActiveUserName DisplayString,
	mtxrHotspotActiveUserDomain DisplayString,
	mtxrHotspotActiveUserIP IpAddress,
	mtxrHotspotActiveUserMAC MacAddress,
	mtxrHotspotActiveUserConnectTime Integer32,
	mtxrHotspotActiveUserValidTillTime Integer32,
	mtxrHotspotActiveUserIdleStartTime Integer32,
	mtxrHotspotActiveUserIdleTimeout Integer32,
	mtxrHotspotActiveUserPingTimeout Integer32,
	mtxrHotspotActiveUserBytesIn Counter64,
	mtxrHotspotActiveUserBytesOut Counter64,
	mtxrHotspotActiveUserPacketsIn Counter64,
	mtxrHotspotActiveUserPacketsOut Counter64,
	mtxrHotspotActiveUserLimitBytesIn Counter64,
	mtxrHotspotActiveUserLimitBytesOut Counter64,
	mtxrHotspotActiveUserAdvertStatus Integer32,
	mtxrHotspotActiveUserRadius Integer32,
	mtxrHotspotActiveUserBlockedByAdvert Integer32
}

mtxrHotspotActiveUserIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 1 }

mtxrHotspotActiveUserServerID OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 2 }

mtxrHotspotActiveUserName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 3 }

mtxrHotspotActiveUserDomain OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 4 }

mtxrHotspotActiveUserIP OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 5 }

mtxrHotspotActiveUserMAC OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 6 }

mtxrHotspotActiveUserConnectTime OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 7 }

mtxrHotspotActiveUserValidTillTime OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 8 }

mtxrHotspotActiveUserIdleStartTime OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 9 }

mtxrHotspotActiveUserIdleTimeout OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 10 }

mtxrHotspotActiveUserPingTimeout OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 11 }

mtxrHotspotActiveUserBytesIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 12 }

mtxrHotspotActiveUserBytesOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 13 }

mtxrHotspotActiveUserPacketsIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 14 }

mtxrHotspotActiveUserPacketsOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 15 }

mtxrHotspotActiveUserLimitBytesIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 16 }

mtxrHotspotActiveUserLimitBytesOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 17 }

mtxrHotspotActiveUserAdvertStatus OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 18 }

mtxrHotspotActiveUserRadius OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 19 }

mtxrHotspotActiveUserBlockedByAdvert OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 20 }

mtxrHotspotActiveUserGroup OBJECT-GROUP OBJECTS {
	mtxrHotspotActiveUserServerID,
	mtxrHotspotActiveUserName,
	mtxrHotspotActiveUserDomain,
	mtxrHotspotActiveUserIP,
	mtxrHotspotActiveUserMAC,
	mtxrHotspotActiveUserConnectTime,
	mtxrHotspotActiveUserValidTillTime,
	mtxrHotspotActiveUserIdleStartTime,
	mtxrHotspotActiveUserIdleTimeout,
	mtxrHotspotActiveUserPingTimeout,
	mtxrHotspotActiveUserBytesIn,
	mtxrHotspotActiveUserBytesOut,
	mtxrHotspotActiveUserPacketsIn,
	mtxrHotspotActiveUserPacketsOut,
	mtxrHotspotActiveUserLimitBytesIn,
	mtxrHotspotActiveUserLimitBytesOut,
	mtxrHotspotActiveUserAdvertStatus,
	mtxrHotspotActiveUserRadius,
	mtxrHotspotActiveUserBlockedByAdvert
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 5 }

-- DHCP ********************************************************************

mtxrDHCPLeaseCount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrDHCP 1 }

mtxrDHCPGroup OBJECT-GROUP OBJECTS {
        mtxrDHCPLeaseCount
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 12 }

-- SYSTEM ********************************************************************

mtxrSystemReboot OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION "set non zero to reboot"
    ::= { mtxrSystem 1 }

mtxrUSBPowerReset OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION "switches off usb power for specified amout of seconds"
    ::= { mtxrSystem 2 }

mtxrSerialNumber OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "RouterBOARD serial number"
    ::= { mtxrSystem 3 }

mtxrFirmwareVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Current firmware version"
    ::= { mtxrSystem 4 }

mtxrNote OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "note"
    ::= { mtxrSystem 5 }

mtxrBuildTime OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "build time"
    ::= { mtxrSystem 6 }

mtxrFirmwareUpgradeVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Upgrade firmware version"
    ::= { mtxrSystem 7 }

mtxrDisplayName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "display name"
    ::= { mtxrSystem 8 }

mtxrBoardName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "board name"
    ::= { mtxrSystem 9 }

mtxrSystemGroup OBJECT-GROUP OBJECTS {
        mtxrSystemReboot,
        mtxrUSBPowerReset,
        mtxrSerialNumber,
        mtxrFirmwareVersion,
        mtxrNote,
        mtxrBuildTime,
        mtxrFirmwareUpgradeVersion,
        mtxrBoardName
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 13 }

-- SCRIPTS ********************************************************************

mtxrScriptTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrScriptTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScripts 1 }

mtxrScriptTableEntry OBJECT-TYPE
    SYNTAX MtxrScriptTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrScriptIndex }
    ::= { mtxrScriptTable 1 }

MtxrScriptTableEntry ::= SEQUENCE {
	mtxrScriptIndex ObjectIndex,
	mtxrScriptName DisplayString,
	mtxrScriptRunCmd Integer32
}

mtxrScriptIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScriptTableEntry 1 }

mtxrScriptName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScriptTableEntry 2 }

mtxrScriptRunCmd OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION "set non zero to run"
    ::= { mtxrScriptTableEntry 3 }

mtxrScriptGroup OBJECT-GROUP OBJECTS {
	mtxrScriptName, mtxrScriptRunCmd
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 8 }

-- SCRIPT RUN *****************************************************************

mtxrScriptRunTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrScriptRunTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "invisible to getnext, accesible only with get request and write premission"
    ::= { mtxrScriptRun 1 }

mtxrScriptRunTableEntry OBJECT-TYPE
    SYNTAX MtxrScriptRunTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrScriptRunIndex }
    ::= { mtxrScriptRunTable 1 }

MtxrScriptRunTableEntry ::= SEQUENCE {
	mtxrScriptRunIndex ObjectIndex,
	mtxrScriptRunOutput DisplayString
}

mtxrScriptRunIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScriptRunTableEntry 1 }

mtxrScriptRunOutput OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "this oid on get request will run script and return it's output"
    ::= { mtxrScriptRunTableEntry 2 }

mtxrScriptRunGroup OBJECT-GROUP OBJECTS {
	mtxrScriptRunOutput
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 21 }

-- Dual Nstreme ***************************************************************

mtxrDnStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrDnStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNstremeDual 1 }

mtxrDnStatEntry OBJECT-TYPE
    SYNTAX MtxrDnStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Nstreme Dual interface"
    INDEX { mtxrDnStatIndex }
    ::= { mtxrDnStatTable 1 }

MtxrDnStatEntry ::= SEQUENCE {
    mtxrDnStatIndex ObjectIndex,
    mtxrDnStatTxRate Gauge32,
    mtxrDnStatRxRate Gauge32,
    mtxrDnStatTxStrength Integer32,
    mtxrDnStatRxStrength Integer32,
    mtxrDnConnected Integer32
}	

mtxrDnStatIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrDnStatEntry 1 }

mtxrDnStatTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrDnStatEntry 2 }

mtxrDnStatRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrDnStatEntry 3 }

mtxrDnStatTxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrDnStatEntry 4 }

mtxrDnStatRxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrDnStatEntry 5 }

mtxrDnConnected OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "0 - not connected, connected otherwise"
    ::= { mtxrDnStatEntry 6 }

mtxrNstremeDualGroup OBJECT-GROUP OBJECTS {
	mtxrDnStatTxRate, mtxrDnStatRxRate,
	mtxrDnStatTxStrength, mtxrDnStatRxStrength, mtxrDnConnected
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 10 }

-- NEIGHBOR *******************************************************************

mtxrNeighborTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrNeighborTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighbor 1 }

mtxrNeighborTableEntry OBJECT-TYPE
    SYNTAX MtxrNeighborTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrNeighborIndex }
    ::= { mtxrNeighborTable 1 }

MtxrNeighborTableEntry ::= SEQUENCE {
	mtxrNeighborIndex ObjectIndex,
	mtxrNeighborIpAddress IpAddress,
	mtxrNeighborMacAddress MacAddress,
	mtxrNeighborVersion DisplayString,
	mtxrNeighborPlatform DisplayString,
	mtxrNeighborIdentity DisplayString,
	mtxrNeighborSoftwareID DisplayString,
        mtxrNeighborInterfaceID ObjectIndex
}

mtxrNeighborIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 1 }

mtxrNeighborIpAddress OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 2 }

mtxrNeighborMacAddress OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 3 }

mtxrNeighborVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 4 }

mtxrNeighborPlatform OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 5 }

mtxrNeighborIdentity OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 6 }

mtxrNeighborSoftwareID OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 7 }

mtxrNeighborInterfaceID OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 8 }

mtxrNeighborGroup OBJECT-GROUP OBJECTS {
	mtxrNeighborIpAddress,
	mtxrNeighborMacAddress,
	mtxrNeighborVersion,
	mtxrNeighborPlatform,
	mtxrNeighborIdentity,
	mtxrNeighborSoftwareID,
	mtxrNeighborInterfaceID
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 11 }

-- GPS ************************************************************************

mtxrDate OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "UNIX time"
    ::= { mtxrGps 1 }

mtxrLongtitude OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "longtitude"
    ::= { mtxrGps 2 }

mtxrLatitude OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "latitude"
    ::= { mtxrGps 3 }

mtxrAltitude OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "altitude"
    ::= { mtxrGps 4 }

mtxrSpeed OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "speed"
    ::= { mtxrGps 5 }

mtxrSattelites OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "visible sattelite count"
    ::= { mtxrGps 6 }

mtxrValid OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "is the data valid"
    ::= { mtxrGps 7 }

mtxrGPSGroup OBJECT-GROUP OBJECTS {
        mtxrDate,
        mtxrLongtitude,
        mtxrLatitude,
        mtxrAltitude,
        mtxrSpeed,
        mtxrSattelites,
        mtxrValid
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 15 }

-- Wireless Modem ************************************************************

mtxrWirelessModemSignalStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "signal strength in dBm (if first ppp-client modem supports)"
    ::= { mtxrWirelessModem 1 }

mtxrWirelessModemSignalECIO OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "signal EC/IO in dB (if first ppp-client modem supports)"
    ::= { mtxrWirelessModem 2 }

mtxrWirelessModemManufacturer OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Modem manufacturer name"
    ::= { mtxrWirelessModem 3 }

mtxrWirelessModemModel OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Modem model name"
    ::= { mtxrWirelessModem 4 }

mtxrWirelessModemRevision OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Modem firmware revision"
    ::= { mtxrWirelessModem 5 }

mtxrWirelessModemIMEI OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Modem serial number"
    ::= { mtxrWirelessModem 6 }

mtxrWirelessModemIMSI OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "International mobile subscriber identity"
    ::= { mtxrWirelessModem 7 }

mtxrWirelessModemAccessTechnology OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Access technology"
    ::= { mtxrWirelessModem 8 }

mtxrWirelessModemFrameErrorRate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Signal frame error rate"
    ::= { mtxrWirelessModem 9 }

mtxrWirelessModemRSRP OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Reference Signal Receive Power"
    ::= { mtxrWirelessModem 10 }

mtxrWirelessModemRSRQ OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Reference Signal Received Quality"
    ::= { mtxrWirelessModem 11 }

mtxrWirelessModemSINR OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Signal-to-Interference-plus-Noise Ratio"
    ::= { mtxrWirelessModem 12 }

mtxrWirelessModemPinStatus OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Pin status of the modem"
    ::= { mtxrWirelessModem 13 }

mtxrWirelessModemGroup OBJECT-GROUP OBJECTS {
        mtxrWirelessModemSignalStrength,
        mtxrWirelessModemSignalECIO,
        mtxrWirelessModemManufacturer,
        mtxrWirelessModemModel,
        mtxrWirelessModemRevision,
        mtxrWirelessModemIMEI,
        mtxrWirelessModemIMSI,
        mtxrWirelessModemAccessTechnology,
        mtxrWirelessModemFrameErrorRate,
        mtxrWirelessModemRSRP,
        mtxrWirelessModemRSRQ,
        mtxrWirelessModemSINR,
        mtxrWirelessModemPinStatus
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 16 }

-- Interface Stats ************************************************************

mtxrInterfaceStatsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrInterfaceStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Extended interface statistics.
    Some interfaces may have only parts of this table
    with unavailable values set to zero."
    ::= { mtxrInterfaceStats 1 }

mtxrInterfaceStatsEntry OBJECT-TYPE
    SYNTAX MtxrInterfaceStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrInterfaceStatsIndex }
    ::= { mtxrInterfaceStatsTable 1 }

MtxrInterfaceStatsEntry ::= SEQUENCE {
    mtxrInterfaceStatsIndex ObjectIndex,
    mtxrInterfaceStatsName DisplayString,

    mtxrInterfaceStatsDriverRxBytes Counter64,
    mtxrInterfaceStatsDriverRxPackets Counter64,
    mtxrInterfaceStatsDriverTxBytes Counter64,
    mtxrInterfaceStatsDriverTxPackets Counter64,

    mtxrInterfaceStatsTxRx64 Counter64,
    mtxrInterfaceStatsTxRx65To127 Counter64,
    mtxrInterfaceStatsTxRx128To255 Counter64,
    mtxrInterfaceStatsTxRx256To511 Counter64,
    mtxrInterfaceStatsTxRx512To1023 Counter64,
    mtxrInterfaceStatsTxRx1024To1518 Counter64,
    mtxrInterfaceStatsTxRx1519ToMax Counter64,

    mtxrInterfaceStatsRxBytes Counter64,
    mtxrInterfaceStatsRxPackets Counter64,
    mtxrInterfaceStatsRxTooShort Counter64,
    mtxrInterfaceStatsRx64 Counter64,
    mtxrInterfaceStatsRx65To127 Counter64,
    mtxrInterfaceStatsRx128To255 Counter64,
    mtxrInterfaceStatsRx256To511 Counter64,
    mtxrInterfaceStatsRx512To1023 Counter64,
    mtxrInterfaceStatsRx1024To1518 Counter64,
    mtxrInterfaceStatsRx1519ToMax Counter64,
    mtxrInterfaceStatsRxTooLong Counter64,
    mtxrInterfaceStatsRxBroadcast Counter64,
    mtxrInterfaceStatsRxPause Counter64,
    mtxrInterfaceStatsRxMulticast Counter64,
    mtxrInterfaceStatsRxFCSError Counter64,
    mtxrInterfaceStatsRxAlignError Counter64,
    mtxrInterfaceStatsRxFragment Counter64,
    mtxrInterfaceStatsRxOverflow Counter64,
    mtxrInterfaceStatsRxControl Counter64,
    mtxrInterfaceStatsRxUnknownOp Counter64,
    mtxrInterfaceStatsRxLengthError Counter64,
    mtxrInterfaceStatsRxCodeError Counter64,
    mtxrInterfaceStatsRxCarrierError Counter64,
    mtxrInterfaceStatsRxJabber Counter64,
    mtxrInterfaceStatsRxDrop Counter64,

    mtxrInterfaceStatsTxBytes Counter64,
    mtxrInterfaceStatsTxPackets Counter64,
    mtxrInterfaceStatsTxTooShort Counter64,
    mtxrInterfaceStatsTx64 Counter64,
    mtxrInterfaceStatsTx65To127 Counter64,
    mtxrInterfaceStatsTx128To255 Counter64,
    mtxrInterfaceStatsTx256To511 Counter64,
    mtxrInterfaceStatsTx512To1023 Counter64,
    mtxrInterfaceStatsTx1024To1518 Counter64,
    mtxrInterfaceStatsTx1519ToMax Counter64,
    mtxrInterfaceStatsTxTooLong Counter64,
    mtxrInterfaceStatsTxBroadcast Counter64,
    mtxrInterfaceStatsTxPause Counter64,
    mtxrInterfaceStatsTxMulticast Counter64,
    mtxrInterfaceStatsTxUnderrun Counter64,
    mtxrInterfaceStatsTxCollision Counter64,
    mtxrInterfaceStatsTxExcessiveCollision Counter64,
    mtxrInterfaceStatsTxMultipleCollision Counter64,
    mtxrInterfaceStatsTxSingleCollision Counter64,
    mtxrInterfaceStatsTxExcessiveDeferred Counter64,
    mtxrInterfaceStatsTxDeferred Counter64,
    mtxrInterfaceStatsTxLateCollision Counter64,
    mtxrInterfaceStatsTxTotalCollision Counter64,
    mtxrInterfaceStatsTxPauseHonored Counter64,
    mtxrInterfaceStatsTxDrop Counter64,
    mtxrInterfaceStatsTxJabber Counter64,
    mtxrInterfaceStatsTxFCSError Counter64,
    mtxrInterfaceStatsTxControl Counter64,
    mtxrInterfaceStatsTxFragment Counter64,
    mtxrInterfaceStatsLinkDowns Counter32,
    mtxrInterfaceStatsTxRx1024ToMax Counter64
}

mtxrInterfaceStatsIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 1 }

mtxrInterfaceStatsName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 2 }

mtxrInterfaceStatsDriverRxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 11 }

mtxrInterfaceStatsDriverRxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 12 }

mtxrInterfaceStatsDriverTxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 13 }

mtxrInterfaceStatsDriverTxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 14 }

mtxrInterfaceStatsTxRx64 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 15 }

mtxrInterfaceStatsTxRx65To127 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 16 }

mtxrInterfaceStatsTxRx128To255 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 17 }

mtxrInterfaceStatsTxRx256To511 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 18 }

mtxrInterfaceStatsTxRx512To1023 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 19 }

mtxrInterfaceStatsTxRx1024To1518 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 20 }

mtxrInterfaceStatsTxRx1519ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 21 }

mtxrInterfaceStatsRxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 31 }
 
mtxrInterfaceStatsRxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 32 }

mtxrInterfaceStatsRxTooShort OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 33 }

mtxrInterfaceStatsRx64 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 34 }

mtxrInterfaceStatsRx65To127 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 35 }

mtxrInterfaceStatsRx128To255 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 36 }

mtxrInterfaceStatsRx256To511 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 37 }

mtxrInterfaceStatsRx512To1023 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 38 }

mtxrInterfaceStatsRx1024To1518 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 39 }

mtxrInterfaceStatsRx1519ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 40 }

mtxrInterfaceStatsRxTooLong OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 41 }

mtxrInterfaceStatsRxBroadcast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 42 }

mtxrInterfaceStatsRxPause OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 43 }

mtxrInterfaceStatsRxMulticast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 44 }

mtxrInterfaceStatsRxFCSError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 45 }

mtxrInterfaceStatsRxAlignError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 46 }

mtxrInterfaceStatsRxFragment OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 47 }

mtxrInterfaceStatsRxOverflow OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 48 }

mtxrInterfaceStatsRxControl OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 49 }

mtxrInterfaceStatsRxUnknownOp OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 50 }

mtxrInterfaceStatsRxLengthError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 51 }

mtxrInterfaceStatsRxCodeError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 52 }

mtxrInterfaceStatsRxCarrierError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 53 }

mtxrInterfaceStatsRxJabber OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 54 }

mtxrInterfaceStatsRxDrop OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 55 }

mtxrInterfaceStatsTxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 61 }

mtxrInterfaceStatsTxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 62 }

mtxrInterfaceStatsTxTooShort OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 63 }

mtxrInterfaceStatsTx64 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 64 }

mtxrInterfaceStatsTx65To127 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 65 }

mtxrInterfaceStatsTx128To255 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 66 }

mtxrInterfaceStatsTx256To511 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 67 }

mtxrInterfaceStatsTx512To1023 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 68 }

mtxrInterfaceStatsTx1024To1518 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 69 }

mtxrInterfaceStatsTx1519ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 70 }

mtxrInterfaceStatsTxTooLong OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 71 }

mtxrInterfaceStatsTxBroadcast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 72 }

mtxrInterfaceStatsTxPause OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 73 }

mtxrInterfaceStatsTxMulticast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 74 }

mtxrInterfaceStatsTxUnderrun OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 75 }

mtxrInterfaceStatsTxCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 76 }

mtxrInterfaceStatsTxExcessiveCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 77 }

mtxrInterfaceStatsTxMultipleCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 78 }

mtxrInterfaceStatsTxSingleCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 79 }

mtxrInterfaceStatsTxExcessiveDeferred OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 80 }

mtxrInterfaceStatsTxDeferred OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 81 }

mtxrInterfaceStatsTxLateCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 82 }

mtxrInterfaceStatsTxTotalCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 83 }

mtxrInterfaceStatsTxPauseHonored OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 84 }

mtxrInterfaceStatsTxDrop OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 85 }

mtxrInterfaceStatsTxJabber OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 86 }

mtxrInterfaceStatsTxFCSError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 87 }

mtxrInterfaceStatsTxControl OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 88 }

mtxrInterfaceStatsTxFragment OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 89 }

mtxrInterfaceStatsLinkDowns OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 90 }

mtxrInterfaceStatsTxRx1024ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 91 }

mtxrInterfaceStatsGroup OBJECT-GROUP OBJECTS {
        mtxrInterfaceStatsName,
        mtxrInterfaceStatsDriverRxBytes,
        mtxrInterfaceStatsDriverRxPackets,
        mtxrInterfaceStatsDriverTxBytes,
        mtxrInterfaceStatsDriverTxPackets,

        mtxrInterfaceStatsTxRx64,
        mtxrInterfaceStatsTxRx65To127,
        mtxrInterfaceStatsTxRx128To255,
        mtxrInterfaceStatsTxRx256To511,
        mtxrInterfaceStatsTxRx512To1023,
        mtxrInterfaceStatsTxRx1024To1518,
        mtxrInterfaceStatsTxRx1519ToMax,

        mtxrInterfaceStatsRxBytes,
        mtxrInterfaceStatsRxPackets,
        mtxrInterfaceStatsRxTooShort,
        mtxrInterfaceStatsRx64,
        mtxrInterfaceStatsRx65To127,
        mtxrInterfaceStatsRx128To255,
        mtxrInterfaceStatsRx256To511,
        mtxrInterfaceStatsRx512To1023,
        mtxrInterfaceStatsRx1024To1518,
        mtxrInterfaceStatsRx1519ToMax,
        mtxrInterfaceStatsRxTooLong,
        mtxrInterfaceStatsRxBroadcast,
        mtxrInterfaceStatsRxPause,
        mtxrInterfaceStatsRxMulticast,
        mtxrInterfaceStatsRxFCSError,
        mtxrInterfaceStatsRxAlignError,
        mtxrInterfaceStatsRxFragment,
        mtxrInterfaceStatsRxOverflow,
        mtxrInterfaceStatsRxControl,
        mtxrInterfaceStatsRxUnknownOp,
        mtxrInterfaceStatsRxLengthError,
        mtxrInterfaceStatsRxCodeError,
        mtxrInterfaceStatsRxCarrierError,
        mtxrInterfaceStatsRxJabber,
        mtxrInterfaceStatsRxDrop,

        mtxrInterfaceStatsTxBytes,
        mtxrInterfaceStatsTxPackets,
        mtxrInterfaceStatsTxTooShort,
        mtxrInterfaceStatsTx64,
        mtxrInterfaceStatsTx65To127,
        mtxrInterfaceStatsTx128To255,
        mtxrInterfaceStatsTx256To511,
        mtxrInterfaceStatsTx512To1023,
        mtxrInterfaceStatsTx1024To1518,
        mtxrInterfaceStatsTx1519ToMax,
        mtxrInterfaceStatsTxTooLong,
        mtxrInterfaceStatsTxBroadcast,
        mtxrInterfaceStatsTxPause,
        mtxrInterfaceStatsTxMulticast,
        mtxrInterfaceStatsTxUnderrun,
        mtxrInterfaceStatsTxCollision,
        mtxrInterfaceStatsTxExcessiveCollision,
        mtxrInterfaceStatsTxMultipleCollision,
        mtxrInterfaceStatsTxSingleCollision,
        mtxrInterfaceStatsTxExcessiveDeferred,
        mtxrInterfaceStatsTxDeferred,
        mtxrInterfaceStatsTxLateCollision,
        mtxrInterfaceStatsTxTotalCollision,
        mtxrInterfaceStatsTxPauseHonored,
        mtxrInterfaceStatsTxDrop,
        mtxrInterfaceStatsTxJabber,
        mtxrInterfaceStatsTxFCSError,
        mtxrInterfaceStatsTxControl,
        mtxrInterfaceStatsTxFragment,
        mtxrInterfaceStatsLinkDowns,
        mtxrInterfaceStatsTxRx1024ToMax
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 17 }

-- POE ************************************************************************

mtxrPOETable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrPOEEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Power Over Ethernet"
    ::= { mtxrPOE 1 }

mtxrPOEEntry OBJECT-TYPE
    SYNTAX MtxrPOEEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrPOEInterfaceIndex }
    ::= { mtxrPOETable 1 }

MtxrPOEEntry ::= SEQUENCE {
    mtxrPOEInterfaceIndex ObjectIndex,
    mtxrPOEName DisplayString,
    mtxrPOEStatus INTEGER,
    mtxrPOEVoltage Voltage,
    mtxrPOECurrent Integer32,
    mtxrPOEPower Power
}

mtxrPOEInterfaceIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPOEEntry 1 }

mtxrPOEName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPOEEntry 2 }

mtxrPOEStatus OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(1),
        waitingForLoad(2),
        poweredOn(3),
        overload(4),
        shortCircuit(5),
        voltageTooLow(6),
        currentTooLow(7),
        powerReset(8),
        voltageTooHigh(9),
        controllerError(10),
        controllerUpgrade(11),
        poeInDetected(12),
        noValidPsu(13),
        controllerInit(14),
        lowVoltageTooLow(15)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPOEEntry 3 }

mtxrPOEVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "V"
    ::= { mtxrPOEEntry 4 }

mtxrPOECurrent OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "mA"
    ::= { mtxrPOEEntry 5 }

mtxrPOEPower OBJECT-TYPE
    SYNTAX Power
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "W"
    ::= { mtxrPOEEntry 6 }

mtxrPOEGroup OBJECT-GROUP OBJECTS {
        mtxrPOEName,
        mtxrPOEStatus,
        mtxrPOEVoltage,
        mtxrPOECurrent,
        mtxrPOEPower
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 18 }

-- LTE Modem ************************************************************

mtxrLTEModemTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrLTEModemEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "LTE Modems"
    ::= { mtxrLTEModem 1 }

mtxrLTEModemEntry OBJECT-TYPE
    SYNTAX MtxrLTEModemEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrLTEModemInterfaceIndex }
    ::= { mtxrLTEModemTable 1 }

MtxrLTEModemEntry ::= SEQUENCE {
    mtxrLTEModemInterfaceIndex ObjectIndex,
    mtxrLTEModemSignalRSSI Integer32,
    mtxrLTEModemSignalRSRQ Integer32,
    mtxrLTEModemSignalRSRP Integer32,
    mtxrLTEModemCellId HexInt,
    mtxrLTEModemAccessTechnology INTEGER,
    mtxrLTEModemSignalSINR Integer32,
    mtxrLTEModemEnbId Integer32,
    mtxrLTEModemSectorId Integer32,
    mtxrLTEModemLac Integer32,
    mtxrLTEModemIMEI DisplayString,
    mtxrLTEModemIMSI DisplayString,
    mtxrLTEModemUICC DisplayString,
    mtxrLTEModemRAT DisplayString
}

mtxrLTEModemInterfaceIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 1 }

mtxrLTEModemSignalRSSI OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrLTEModemEntry 2 }

mtxrLTEModemSignalRSRQ OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dB"
    ::= { mtxrLTEModemEntry 3 }

mtxrLTEModemSignalRSRP OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrLTEModemEntry 4 }

mtxrLTEModemCellId OBJECT-TYPE
    SYNTAX HexInt
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "current cell ID"
    ::= { mtxrLTEModemEntry 5 }

mtxrLTEModemAccessTechnology OBJECT-TYPE
    SYNTAX INTEGER {
        unknown(-1),
        gsmcompact(0),
        gsm(1),
        utran(2),
        egprs(3),
        hsdpa(4),
        hsupa(5),
        hsdpahsupa(6),
        eutran(7),
        nr-sa(11),
        nr-nsa(13)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "as reported by +CREG"
    ::= { mtxrLTEModemEntry 6 }

mtxrLTEModemSignalSINR OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dB"
    ::= { mtxrLTEModemEntry 7 }

mtxrLTEModemEnbId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 8 }

mtxrLTEModemSectorId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 9 }

mtxrLTEModemLac OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 10 }

mtxrLTEModemIMEI OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 11 }

mtxrLTEModemIMSI OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 12 }

mtxrLTEModemUICC OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 13 }

mtxrLTEModemRAT OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 14 }

mtxrLTEModemGroup OBJECT-GROUP OBJECTS {
        mtxrLTEModemSignalRSSI,
        mtxrLTEModemSignalRSRQ,
        mtxrLTEModemSignalRSRP,
        mtxrLTEModemCellId,
        mtxrLTEModemAccessTechnology,
        mtxrLTEModemSignalSINR,
        mtxrLTEModemEnbId,
        mtxrLTEModemSectorId,
        mtxrLTEModemLac,
        mtxrLTEModemIMEI,
        mtxrLTEModemIMSI,
        mtxrLTEModemUICC,
        mtxrLTEModemRAT
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 19 }

-- Partition ************************************************************

mtxrPartitionTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrPartitionEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "system partitions"
    ::= { mtxrPartition 1 }

mtxrPartitionEntry OBJECT-TYPE
    SYNTAX MtxrPartitionEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrPartitionIndex }
    ::= { mtxrPartitionTable 1 }

MtxrPartitionEntry ::= SEQUENCE {
    mtxrPartitionIndex ObjectIndex,
    mtxrPartitionName DisplayString,
    mtxrPartitionSize Integer32,
    mtxrPartitionVersion DisplayString,
    mtxrPartitionActive BoolValue,
    mtxrPartitionRunning BoolValue
}

mtxrPartitionIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPartitionEntry 1 }

mtxrPartitionName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPartitionEntry 2 }

mtxrPartitionSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "MB"
    ::= { mtxrPartitionEntry 3 }

mtxrPartitionVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPartitionEntry 4 }

mtxrPartitionActive OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPartitionEntry 5 }

mtxrPartitionRunning OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPartitionEntry 6 }

mtxrPartitionGroup OBJECT-GROUP OBJECTS {
        mtxrPartitionName,
        mtxrPartitionSize,
        mtxrPartitionVersion,
        mtxrPartitionActive,
        mtxrPartitionRunning
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 20 }

-- OPTICAL *****************************************************************

mtxrOpticalTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrOpticalTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "SFP and GPON information"
    ::= { mtxrOptical 1 }

mtxrOpticalTableEntry OBJECT-TYPE
    SYNTAX MtxrOpticalTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrOpticalIndex }
    ::= { mtxrOpticalTable 1 }

MtxrOpticalTableEntry ::= SEQUENCE {
	mtxrOpticalIndex ObjectIndex,
        mtxrOpticalName DisplayString,
        mtxrOpticalRxLoss BoolValue,
        mtxrOpticalTxFault BoolValue,
        mtxrOpticalWavelength GDiv100,
        mtxrOpticalTemperature Gauge32,
        mtxrOpticalSupplyVoltage GDiv1000,
        mtxrOpticalTxBiasCurrent Gauge32,
        mtxrOpticalTxPower IDiv1000,
        mtxrOpticalRxPower IDiv1000,
        mtxrOpticalVendorName DisplayString,
        mtxrOpticalVendorSerial DisplayString

}

mtxrOpticalGroup OBJECT-GROUP OBJECTS {
        mtxrOpticalName,
        mtxrOpticalRxLoss,
        mtxrOpticalTxFault,
        mtxrOpticalWavelength,
        mtxrOpticalTemperature,
        mtxrOpticalSupplyVoltage,
        mtxrOpticalTxBiasCurrent,
        mtxrOpticalTxPower,
        mtxrOpticalRxPower,
        mtxrOpticalVendorName,
        mtxrOpticalVendorSerial
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 6 }

mtxrOpticalIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 1 }

mtxrOpticalName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 2 }

mtxrOpticalRxLoss OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 3 }

mtxrOpticalTxFault OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 4 }

mtxrOpticalWavelength OBJECT-TYPE
    SYNTAX GDiv100
    UNITS "nm"
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 5 }

mtxrOpticalTemperature OBJECT-TYPE
    SYNTAX Gauge32
    UNITS "C"
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 6 }

mtxrOpticalSupplyVoltage OBJECT-TYPE
    SYNTAX GDiv1000
    UNITS "V"
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 7 }

mtxrOpticalTxBiasCurrent OBJECT-TYPE
    SYNTAX Gauge32
    UNITS "mA"
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 8 }

mtxrOpticalTxPower OBJECT-TYPE
    SYNTAX IDiv1000
    UNITS "dBm"
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 9 }

mtxrOpticalRxPower OBJECT-TYPE
    SYNTAX IDiv1000
    UNITS "dBm"
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 10 }

mtxrOpticalVendorName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 11 }

mtxrOpticalVendorSerial OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrOpticalTableEntry 12 }

-- IPSec *****************************************************************

mtxrIkeSACount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "IKE SA count"
    ::= { mtxrIPSec 1 }

mtxrIkeSATable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrIkeSATableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "IKE SA table"
    ::= { mtxrIPSec 2 }

mtxrIkeSATableEntry OBJECT-TYPE
    SYNTAX MtxrIkeSATableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX {
        mtxrIkeSAIndex
    }
    ::= { mtxrIkeSATable 1 }

MtxrIkeSATableEntry ::= SEQUENCE {
        mtxrIkeSAIndex ObjectIndex,
        mtxrIkeSAInitiatorCookie IsakmpCookie,
        mtxrIkeSAResponderCookie IsakmpCookie,
        mtxrIkeSAResponder BoolValue,
        mtxrIkeSANatt BoolValue,
        mtxrIkeSAVersion Gauge32,
        mtxrIkeSAState INTEGER,
        mtxrIkeSAUptime TimeTicks,
        mtxrIkeSASeen TimeTicks,
        mtxrIkeSAIdentity DisplayString,
        mtxrIkeSAPh2Count Gauge32,
        mtxrIkeSALocalAddressType InetAddressType,
        mtxrIkeSALocalAddress InetAddress,
        mtxrIkeSALocalPort InetPortNumber,
        mtxrIkeSAPeerAddressType InetAddressType,
        mtxrIkeSAPeerAddress InetAddress,
        mtxrIkeSAPeerPort InetPortNumber,
        mtxrIkeSADynamicAddressType InetAddressType,
        mtxrIkeSADynamicAddress InetAddress,
        mtxrIkeSATxBytes Counter64,
        mtxrIkeSARxBytes Counter64,
        mtxrIkeSATxPackets Counter64,
        mtxrIkeSARxPackets Counter64
}

mtxrIkeSAGroup OBJECT-GROUP OBJECTS {
        mtxrIkeSACount,
        mtxrIkeSAInitiatorCookie,
        mtxrIkeSAResponderCookie,
        mtxrIkeSAResponder,
        mtxrIkeSANatt,
        mtxrIkeSAVersion,
        mtxrIkeSAState,
        mtxrIkeSAUptime,
        mtxrIkeSASeen,
        mtxrIkeSAIdentity,
        mtxrIkeSAPh2Count,
        mtxrIkeSALocalAddressType,
        mtxrIkeSALocalAddress,
        mtxrIkeSALocalPort,
        mtxrIkeSAPeerAddressType,
        mtxrIkeSAPeerAddress,
        mtxrIkeSAPeerPort,
        mtxrIkeSADynamicAddressType,
        mtxrIkeSADynamicAddress,
        mtxrIkeSATxBytes,
        mtxrIkeSARxBytes,
        mtxrIkeSATxPackets,
        mtxrIkeSARxPackets
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 7 }

mtxrIkeSAIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 1 }

mtxrIkeSAInitiatorCookie OBJECT-TYPE
    SYNTAX IsakmpCookie
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "initiator SPI"
    ::= { mtxrIkeSATableEntry 2 }

mtxrIkeSAResponderCookie OBJECT-TYPE
    SYNTAX IsakmpCookie
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "responder SPI"
    ::= { mtxrIkeSATableEntry 3 }

mtxrIkeSAResponder OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "IKE side"
    ::= { mtxrIkeSATableEntry 4 }

mtxrIkeSANatt OBJECT-TYPE
    SYNTAX BoolValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "NAT is detected"
    ::= { mtxrIkeSATableEntry 5 }

mtxrIkeSAVersion OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "protocol version"
    ::= { mtxrIkeSATableEntry 6 }

mtxrIkeSAState OBJECT-TYPE
    SYNTAX INTEGER {
        exchange(1),
        established(2),
        expired(3),
        eap(4)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 7 }

mtxrIkeSAUptime OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 8 }

mtxrIkeSASeen OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "time elapsed since last valid IKE packet"
    ::= { mtxrIkeSATableEntry 9 }

mtxrIkeSAIdentity OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "peer identity"
    ::= { mtxrIkeSATableEntry 10 }

mtxrIkeSAPh2Count OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "total ph2 SA pairs"
    ::= { mtxrIkeSATableEntry 11 }

mtxrIkeSALocalAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 12 }

mtxrIkeSALocalAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 13 }

mtxrIkeSALocalPort OBJECT-TYPE
    SYNTAX InetPortNumber
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 14 }

mtxrIkeSAPeerAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 15 }

mtxrIkeSAPeerAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 16 }

mtxrIkeSAPeerPort OBJECT-TYPE
    SYNTAX InetPortNumber
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 17 }

mtxrIkeSADynamicAddressType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrIkeSATableEntry 18 }

mtxrIkeSADynamicAddress OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dynamic address allocated by mode config"
    ::= { mtxrIkeSATableEntry 19 }

mtxrIkeSATxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "ph2 SA tx bytes"
    ::= { mtxrIkeSATableEntry 20 }

mtxrIkeSARxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "ph2 SA rx bytes"
    ::= { mtxrIkeSATableEntry 21 }

mtxrIkeSATxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "ph2 SA tx packets"
    ::= { mtxrIkeSATableEntry 22 }

mtxrIkeSARxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "ph2 SA rx packets"
    ::= { mtxrIkeSATableEntry 23 }

mtxrWifiCapsman OBJECT IDENTIFIER ::= { mtxrWifi 1 }

mtxrWifiCapsmanEnabled OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Indicates whether the Capsman is enabled."
    ::= { mtxrWifiCapsman 1 }

mtxrWifiCapsmanInterfaces OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "List of interfaces associated with Capsman."
    ::= { mtxrWifiCapsman 2 }

mtxrWifiCapsmanCACertificate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "The CA certificate used by Capsman."
    ::= { mtxrWifiCapsman 3 }

mtxrWifiCapsmanCertificate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "The local certificate used by Capsman."
    ::= { mtxrWifiCapsman 4 }

mtxrWifiCapsmanRequirePeerCertificate OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Whether a peer certificate is required."
    ::= { mtxrWifiCapsman 5 }

mtxrWifiCapsmanPackagePath OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Path to the Capsman package directory."
    ::= { mtxrWifiCapsman 6 }

mtxrWifiCapsmanUpgradePolicy OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Capsman upgrade policy."
    ::= { mtxrWifiCapsman 7 }

mtxrWifiCapsmanGeneratedCaCertificate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Automatically generated CA certificate."
    ::= { mtxrWifiCapsman 8 }

mtxrWifiCapsmanGeneratedCertificate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Automatically generated local certificate."
    ::= { mtxrWifiCapsman 9 }

mtxrWifiCap OBJECT IDENTIFIER ::= { mtxrWifi 2 }

mtxrCapEnabled OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Indicates whether the CAP is enabled."
    ::= { mtxrWifiCap 1 }

mtxrCapInterfaces OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "List of interfaces used by the CAP."
    ::= { mtxrWifiCap 2 }

mtxrCapCertificate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "The local certificate used by the CAP."
    ::= { mtxrWifiCap 3 }

mtxrCapCapsManAddresses OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Addresses of associated CapsMan controllers."
    ::= { mtxrWifiCap 4 }

mtxrCapCapsManNames OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Names of associated CapsMan controllers."
    ::= { mtxrWifiCap 5 }

mtxrCapCapsManCertificateCommonNames OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Common names of CapsMan certificates."
    ::= { mtxrWifiCap 6 }

mtxrCapLockToCapsMan OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Indicates if the CAP is locked to a specific CapsMan."
    ::= { mtxrWifiCap 7 }

mtxrCapSlavesStatic OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Indicates if CAP slaves are set to static mode."
    ::= { mtxrWifiCap 8 }

mtxrCapSlavesDatapath OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Datapath configuration of CAP slaves."
    ::= { mtxrWifiCap 9 }

mtxrCapRequestedCertificate OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Requested certificate for the CAP."
    ::= { mtxrWifiCap 10 }

mtxrCapLockedCapsManCommonName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Locked CapsMan common name."
    ::= { mtxrWifiCap 11 }

mtxrCapCurrentCapsManAddress OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Current CapsMan address being used."
    ::= { mtxrWifiCap 12 }

mtxrCapCurrentCapsManIdentity OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Current identity of the connected CapsMan."
    ::= { mtxrWifiCap 13 }

-- Remote Caps *************************************************

mtxrRemoteCapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWifiRemoteCapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWifi 3 }

mtxrWifiRemoteCapEntry OBJECT-TYPE
    SYNTAX MtxrWifiRemoteCapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Entry containing remote CAP statistics"
    INDEX { mtxrRemoteCapId }
    ::= { mtxrRemoteCapTable 1 }

MtxrWifiRemoteCapEntry ::= SEQUENCE {
    mtxrRemoteCapId                ObjectIndex,
    mtxrRemoteCapAddress           DisplayString,
    mtxrRemoteCapIdentity          DisplayString,
    mtxrRemoteCapBoardName         DisplayString,
    mtxrRemoteCapSerial            DisplayString,
    mtxrRemoteCapVersion           DisplayString,
    mtxrRemoteCapBaseMac           MacAddress,
    mtxrRemoteCapCommonName        DisplayString,
    mtxrRemoteCapState             DisplayString
}

mtxrRemoteCapId OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "ID of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 1 }

mtxrRemoteCapAddress OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "IP address of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 2 }

mtxrRemoteCapIdentity OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Identity name of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 3 }

mtxrRemoteCapBoardName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Board name of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 4 }

mtxrRemoteCapSerial OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Serial number of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 5 }

mtxrRemoteCapVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "RouterOS version of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 6 }

mtxrRemoteCapBaseMac OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Base MAC address of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 7 }

mtxrRemoteCapCommonName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Certificate common name of the remote CAP."
    ::= { mtxrWifiRemoteCapEntry 8 }

mtxrRemoteCapState OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "State of the remote CAP (e.g., connected, disconnected)."
    ::= { mtxrWifiRemoteCapEntry 9 }
    
-- Wifi Registration Table *************************************************

mtxrWifiRegistrationTable        OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWifiRegistrationTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWifi 4 }

mtxrWifiRegistrationTableEntry OBJECT-TYPE
    SYNTAX MtxrWifiRegistrationTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Entry containing wifi registration statistics"
    INDEX { mtxrWifiRegistrationMacAddress, mtxrWifiRegistrationInterface }
    ::= { mtxrWifiRegistrationTable 1 }

MtxrWifiRegistrationTableEntry ::= SEQUENCE {
    mtxrWifiRegistrationMacAddress         MacAddress,
    mtxrWifiRegistrationInterface          ObjectIndex,
    mtxrWifiRegistrationSsid               DisplayString,
    mtxrWifiRegistrationUptime             TimeTicks,
    mtxrWifiRegistrationLastActivity       Integer32,
    mtxrWifiRegistrationSignal             Integer32,
    mtxrWifiRegistrationAuthType           DisplayString,
    mtxrWifiRegistrationBand               DisplayString,
    mtxrWifiRegistrationTxRate             Gauge32,
    mtxrWifiRegistrationRxRate             Gauge32,
    mtxrWifiRegistrationTxPackets          Counter64,
    mtxrWifiRegistrationRxPackets          Counter64,
    mtxrWifiRegistrationTxBytes            Counter64,
    mtxrWifiRegistrationRxBytes            Counter64,
    mtxrWifiRegistrationTxBitsPerSecond    Integer32,
    mtxrWifiRegistrationRxBitsPerSecond    Integer32,
    mtxrWifiRegistrationVlanId             Integer32,
    mtxrWifiRegistrationAuthorized         TruthValue
}

mtxrWifiRegistrationMacAddress OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "MAC address of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 1 }

mtxrWifiRegistrationInterface OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Interface id of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 2 }

mtxrWifiRegistrationSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "SSID of the connected access point."
    ::= { mtxrWifiRegistrationTableEntry 3 }

mtxrWifiRegistrationUptime OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Uptime of the registered connection."
    ::= { mtxrWifiRegistrationTableEntry 4 }

mtxrWifiRegistrationLastActivity OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Time since the last activity of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 5 }

mtxrWifiRegistrationSignal OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Signal strength of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 6 }

mtxrWifiRegistrationAuthType OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Authentication type used by the registered device."
    ::= { mtxrWifiRegistrationTableEntry 7 }

mtxrWifiRegistrationBand OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Wireless band used by the registered device."
    ::= { mtxrWifiRegistrationTableEntry 8 }

mtxrWifiRegistrationTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Transmission rate of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 9 }

mtxrWifiRegistrationRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Reception rate of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 10 }

mtxrWifiRegistrationTxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Number of transmitted packets."
    ::= { mtxrWifiRegistrationTableEntry 11 }

mtxrWifiRegistrationRxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Number of received packets."
    ::= { mtxrWifiRegistrationTableEntry 12 }

mtxrWifiRegistrationTxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Number of transmitted bytes."
    ::= { mtxrWifiRegistrationTableEntry 13 }

mtxrWifiRegistrationRxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Number of received bytes."
    ::= {mtxrWifiRegistrationTableEntry 14 }

mtxrWifiRegistrationTxBitsPerSecond OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Transmission rate in bits per second."
    ::= { mtxrWifiRegistrationTableEntry 15 }

mtxrWifiRegistrationRxBitsPerSecond OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Reception rate in bits per second."
    ::= { mtxrWifiRegistrationTableEntry 16 }

mtxrWifiRegistrationVlanId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "VLAN ID of the registered device."
    ::= { mtxrWifiRegistrationTableEntry 17 }

mtxrWifiRegistrationAuthorized OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Indicates whether the device is authorized."
    ::= { mtxrWifiRegistrationTableEntry 18 }

-- Wifi Interfaces ***********************************************

mtxrWifiInterfaces        OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWifiInterfacesEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWifi 5 }

mtxrWifiInterfacesEntry OBJECT-TYPE
    SYNTAX MtxrWifiInterfacesEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "An entry representing WiFi interface"
    INDEX { mtxrWifiInterfacesId }
    ::= { mtxrWifiInterfaces 1 }

MtxrWifiInterfacesEntry ::= SEQUENCE {
    mtxrWifiInterfacesId             ObjectIndex,
    mtxrWifiInterfacesName           DisplayString,
    mtxrWifiInterfacesSsid           DisplayString,
    mtxrWifiInterfacesFreq           DisplayString
}

mtxrWifiInterfacesId OBJECT-TYPE
    SYNTAX      ObjectIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Unique identifier for each WiFi interface"
    ::= { mtxrWifiInterfacesEntry 1 }

mtxrWifiInterfacesName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Name of the WiFi interface"
    ::= { mtxrWifiInterfacesEntry 2 }

mtxrWifiInterfacesSsid OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "SSID associated with the WiFi interface"
    ::= { mtxrWifiInterfacesEntry 3 }

mtxrWifiInterfacesFreq OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Frequency used by the WiFi interface"
    ::= { mtxrWifiInterfacesEntry 4 }

-- TRAPS **********************************************************************

mtxrNotifications OBJECT IDENTIFIER ::= { mtxrTraps 0 }

mtxrTrap NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION "Mikrotik trap OID"
    ::= { mtxrNotifications 1 }

mtxrTemperatureException NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "Mikrotik CPU temperature exception trap"
    ::= { mtxrNotifications 2 }

mtxrTrapGroup NOTIFICATION-GROUP NOTIFICATIONS {
        mtxrTrap,
        mtxrTemperatureException
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 14 }

-- Connection Tracking ********************************************************

mtxrCtTotalEntries OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Total number of connections"
    ::= { mtxrCT 1 }

mtxrCtIP4Entries OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Total number of ipv4 connections"
    ::= { mtxrCT 2 }

mtxrCtIP6Entries OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Total number of ipv6 connections"
    ::= { mtxrCT 3 }

-- ***************************************************************************

END

